# UCP ClickCall

The ClickCall service is the first open web service Ericsson-LG add to iPECS UCP. It is very basic and only holds one function, an external application can make a device that uses the IPKTU protocol dial any number.

This may not sound like much, but actually means you can do a lot of things. You can obviously call an internal or external number, but you can also activate features that uses codes dnd, forwarding and so on.

# Programming

To activate ClickCall you need to enable the service in pgm 111 and associate it with a station in pgm 443. Let us see what you need to do to activate ClickCall on station 409, a LIP-8024E.

Start to check what port the service is running on. The default port is 7878.

This is a basic UCP ClickCall test form that can be used to test the web service. Before you can use this feature you need to port forward 7878 to your UCP.